Arachne PPP Wizard - modem commands I need some information about your modem and your telephone line. We have to determine two commands, which MINITERM has to say to your modem. First is called Init string, and for most modems, it will be simply ATZ or AT&F0. Unfortunately, although all modems will respond OK to ATZ, not all of them will work correctly after such init string.
Please enter init string for your modem: The second command used by MINITERM is called Dial command:

Tone dial, wait for dialtone (ATDT) | Pulse dial, wait for dialtone (ATDP) Dialtone is usually available in USA and other Western countries.
Tone dial, no dialtone (ATX3DT) | Pulse dial, no dialtone (ATX3DP)
"No dialtone" option is often required in Central and Eastern Europe