Arachne PPP Wizard - communication speed Now we must decide, how fast can Arachne components MINITERM and DOSPPPD talk to your modem. This communication speed is always higher, than the real modem speed, so if you have 14400 bps (14k4) modem, you should choose communication speed at least 19200 bps, for 33600 bps (33k6) modem choose 38400 bps, etc. Historical PCs used to have speed of COM1 and COM2 ports limited to 9600 bps.
Please select communication speed:

< 9600 bps | < 19200 bps | < 38400 bps | < 115200 bps