This is very experimental, unofficial build of CTMOUSE 1.8 beta 8 by
Arachne Labs.

It returns Microsoft Intellimouse compatible (eg. Genius Netscoll+) wheel
status in BH (high byte of BX register) when serivce AX=0x03 of INT 0x33
is called, which should be compatible with most existing DOS library
functions returning mouse buttons status, available for most programming
languages. BH values 0xf to 0xa indicate movement in one direction, values
0x1 to 0x7 indicate movent in oposite direction. Event queuing and service
AX=0x11 support are not yet implemented, and will be probably included in
official CTMOUSE 1.9 release, as promised by CTMOUSE development team.

You have to replace your mouse driver in AUTOEXEC.BAT by CTMOUSE driver.
It should be able to autodetect mouse type on any serial port.

Please contact netdave@arachne.cz for further information about this CTMOUSE
patch.


